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DEFINITION OF THE ISSUE:

When using Touchstone data to define models, it is essential to know how the ports of that Touchstone data set should be connected in a design.  This implies that the “port ordering” or “port mapping” information must be supplied along with or inside the Touchstone file.  Currently, this is information is sometimes provided in a separate file, but increasingly more often it is included in the Touchstone file as a commented “header” section.

When a Touchstone file contains many ports, connecting its ports manually becomes a tedious and error-prone job.  Consequently, automation is highly desired.  EDA vendors developed several different formats throughout the years, but the problem is that they are all different with various features and capabilities, making parsing them difficult.  Additionally, in most cases this information is provided as a commented header section in the Touchstone file, and strictly speaking, comments are non-parsable, arbitrary text.

The goal of this proposal is to provide a standardized port mapping format for Touchstone files so that all relevant information could be included in it, and all EDA tools could parse them reliably.




SOLUTION REQUIREMENTS:

Port Mapping structures and data must be able to support:
1. Reliably, hooking up a Touchstone File in a simulation.
2. Automate creating a schematic symbol.
3. Automate generating/verifying [Interconnect Model]s in .ibs files.
4. Automate generating/verifying [EMD Model]s in .emd files. 
5. Automate generating/verifying [C Comp Model]s in .ibs files.
6. Enable Touchstone File viewers to generate mixed-mode network parameters for differential ports.
7. Report Sij Status (Measured | Simulated | TBD | Placeholder)
8. Automatic generation of test probe locations for test equipment.
9. Support swathing  
10. Ability to add new user defined parameters


The Touchstone specification must meet these requirements:
Table 1: Solution Requirements
	Requirement
	Notes

	1. Define two new keywords
	[Begin Port Map] / [End Port Map]

	2. Define connections to IBIS structures
	EMD, IBIS Interconnect, C_comp_model, Ts4file

	3. Define structures for connectivity as well as for data and schematic display
	Physical, Logical, Diff_port, and Net structures






SUMMARY OF PROPOSED CHANGES:
For review purposes, the proposed changes are summarized as follows:
Table 2: Touchstone Keywords Affected
	Specification Item
	New/Modified/Other
	Notes

	[Begin Port Map] / [End Port Map]
	New
	New keywords are self-contained and only interact with the [Number of Ports] keyword




PROPOSED CHANGES:
Add the following keywords to the Touchstone specification in the appropriate location:



Keyword:	[Begin Port Map] / [End Port Map]
Required:	Optional; illegal prior to Version 3.0.
Description:	Identifies and associates physical, schematic, and/or measurement locations with the port numbers specified in a Touchstone file
Sub-Params:	Data_usage, Group, Port, Source, Swathing, Symbol_leftside, Symbol_topside, Symbol_rightside, Symbol_bottomside, UD, Unit
Usage rules:	If present in the file, the [Begin Port Map] / [End Port Map] keyword pair shall immediately follow the [Number of Ports] keyword and its associated data.  Each subparameter shall start on a new line.

	Data_usage is an optional, informative subparameter which takes a single string argument.  The subparameter identifies instances wherethat the Touchstone file is intended to be used as data representings part of a larger structure for simulation.  The permitted string arguments are listed below.  Only one Data_usage entry is permitted per [Begin Port Map]/[End Port Map] keyword pair.

“IBIS_Interconnect” – this indicates that the Touchstone data represents part of an IBIS [Interconnect Model].

“EMD” – this indicates that the Touchstone file represents part of an IBIS [EMD Model].

[bookmark: _Hlk176265751]“C_comp_model” – this indicates that the Touchstone file represents an IBIS [C Comp Model].

“Ts4file” – this indicates that the Touchstone file represents the complex impedance of a buffer as described in an IBIS AMI file.

	If Data_usage is present for a given Port Map, a Physical name-value pair (see below) shall be present for each Port in that Port Map.

The Source subparameter is optional.  It is followed by a file name identifying the original file where the Touchstone data was obtained or derived.  The file name may be an ODB++ board data base, a schematic file, a simulation model, or any other data file.  As the subparameter is purely informational, the data file is not required to be present on the computer system containing the associated Touchstone file.

The Swathing subparameter is optional.  It is followed by a string, defining a Schema name.  Connector companies may create Touchstone files for a portion or “slice” of a connector.  These “slices” may be combined algorithmically according to the schema to create a virtual Touchstone file that represents all the pins of the connector.  Reserved Schemas, defined in a separate specification, are supported, as are other, model-maker-defined Schema values.

The Group subparameter is optional.  The Group subparameter describes collections of power and ground physical locations.  Group may appear multiple times for a [Begin Port Map]/[End Port Map] pair, with each Group subparameter appearing on a separate line.  These lines are placed after the last Port subparameter (see below) and before the [End Port Map] keyword.  The Group subparameter is followed by the name “Physical” and the name of the Group whose port is described by the line; these strings are separated by white space.  The Group <name> is followed by white space, a “(“, followed by a list of Physical names, and terminated by a “)”.  Any Physical names (see below) associated with Ports of Type Signal shall not be used as Group names.  A line termination sequence without a “)” continues the list of Physical names on the next line.  Physical names shall not contain white space.  Group names shall only contain alphanumeric characters and the underscore (“_”) character; the period (“.”) character is prohibited in Group names.	Comment by Mirmak, Michael: Need description of what Group *is*: power and ground terminals.

The Symbol_* subparameters are intended to provide guidance on the placement of ports on a circuit element or symbol representing the Touchstone data in a larger schematic diagram (e.g., so that symbols may be automatically generated by an EDA tool). 

The Symbol_leftside subparameter is optional.  This subparameter shall appear on a separate line after the last Port subparameter and before the [End Port Map] keyword.  The Symbol_leftside subparameter string is followed by a list of Port numbers defining terminals to be shown on the left side of a schematic symbol, ordered as listed from top to bottom.

The Symbol_rightside subparameter is optional.  This subparameter shall appear on a separate line  after the last Port subparameter and before the [End Port Map] keyword.  The Symbol_rightside subparameter string is followed by a list of Port numbers defining terminals to be shown on the right side of a schematic symbol, ordered as listed from top to bottom.

The Symbol_topside subparameter is optional.  This subparameter shall appear on a separate line after the last Port subparameter and before the [End Port Map] keyword.  The Symbol_topside subparameter string is followed by a list of Port numbers defining terminals to be shown on the top side of a schematic symbol, ordered as listed from left to right.

The Symbol_bottomside subparameter is optional.  This subparameter shall appear on a separate line after the last Port subparameter and before the [End Port Map] keyword.  The Symbol_bottomside subparameter string is followed by a list of Port numbers defining terminals to be shown on the bottom side of a schematic symbol, ordered as listed from left to right.

For all Symbol_* subparameters above, the Port number arguments need not follow a particular numerical order, but the sequence of Port numbers shall correspond to the physical placement of the port numbers in the symbol in the orientation described (e.g., for Symbol_leftside, Port arguments 1, 3, 7, 10, 6 defines Port 1 as being the topmost port and Port 6 as being the bottommost port).

If any Symbol_leftside, Symbol_rightside, Symbol_topside or Symbol_bottomside subparameters are present then any Port number shall appear once and only once in these subparameters.

The Unit subparameter is optional in most cases (see below).  The “Unit” string shall be followed by a string declaring the unit for physical coordinates.  The only permitted arguments are “m”, “mm”, “microns”, “inches”, and “mils”,  for meters, millimeters, microns, inches, and mils, respectively.  The Unit subparameter shall be present when any coordinate-based definitions are used for Physical port descriptions.

The UD (for user-defined) subparameter is optional.  Note that user-defined information may be declared after the Port declarations or in Port lines.  When used after the Port declarations, “UD” is considered a subparameter and UD data shall be declared using lines, without parentheses, where an arbitrary number of strings may follow the “UD” string and whitespace.  For UD data on Port lines, the data shall follow the string “UD” and whitespace within the same pair of parentheses.  UD information in either location effectively will be ignored by EDA tools, but may be used to track how the data describing the port behavior was generated, and/or how the Port data was physically measured.

The Port subparameter is required.  The [Begin Port Map] keyword shall be followed by as many Port subparameter lines as the number of ports defined by the [Number of Ports] keyword.  The entire content of each Port subparameter shall be on a single line.  Note that a Port always denotes a pair of terminals; the reference terminal may be explicitly identified using the syntax defined below or, if not explicitly identified, is assumed to be A_gnd. 

The Port subparameter shall be followed by whitespace and an integer number, indicating which port is described by the line.  Note that the listed Port numbers shall include all positive, non-zero integers from one (“1”) to N inclusive, where N is equal to the Number of Ports entry in the same Touchstone file.    Ports may be listed in any order so long as no Port number is duplicated.  The integer port number is followed by whitespace, then (<name> <value>) pairs, hereafter called “name-value pairs”, enclosed in parentheses as shown.  In addition, the character “-“ may be used before specific name-value pairs as described below.  Unless otherwise noted, all Port name-value pairs are optional.  Names used on the Port lines are case-sensitive.  	Comment by Author: Port 0 not accepted; shall be less than or equal to the number of ports entry in TS file above.

The strings below are reserved and shall not be used as values in name-value pairs for the Port subparameter:

	Diff_port
	Logical
	Net
	Physical
	Probe
	Side
	Type
	UD

The Port subparameter string and its associated Port number shall appear first, at the beginning of each line.  Name-value pairs may appear in any order thereafter.

Several name-value pairs refer to the port as a unit.  These name-value pairs may only appear once per Port line.  These are:

	Diff_port
	Side
	Type
	UD

Several name-value pairs define properties of individual terminals; they apply to terminals within the port, not to the port as a whole.  These name-value pairs may appear twice per Port line; if one of these name-value pairs appears twice for a specific port, one of those  name-value pairs shall be preceded by the “-“ character.  The terminal-oriented names are:

	Logical
	Net
	Physical
	Probe

The “-“ symbol is used to associate these name-value pairs with the reference terminal of the port; the “-“ symbol may also be used with a Physical Group of terminals.  Use of these name-value pairs without the “-“ symbol indicates the pair refers to the measured terminal, not its reference.    

	Port n (name value) (name value)  -(name value)  (name value) -(name value)	Comment by Mirmak, Michael: Diff_port, Side, Type in this case

where n is the non-zero positive integer port number, and name is one of the reserved Port names listed above.  

The port-oriented names Diff_port, Side, and Type shall not appear in a name-value pair identified with “-“. 

Note that the “-“ symbol shall be followed without whitespace by the “(“ character in its associated name-value pair.  The parentheses defining a name-value pair may be separated from other parts of the Port line with whitespace.

If the “–“ symbol is not present for a port, the reference terminal for that port is connected to A_gnd.  Note that A_gnd may not appear for the Logical, Net, Physical, or Probe name-value pairs associated with the non-reference terminal of a Port.

	Examples:

Port 1 (Physical U7.1)
Port 2 (Type S) (Physical U7.2)

Port 3 (Physical U7.4) (Logical DQS+)  (Diff_port 4)  -(Physical U7.3local_reference)
Port 4 (Physical U7.5) (Logical DQS-)   (Diff_port 3)  -(Physical local_referenceU7.6) 	Comment by Mirmak, Michael: Does this need a “-”?  And should this and Port 3 have Reference? 


	Port Name-Value Pair Rules

	Note that all name-value pairs described below are optional.  None of the name-value pairs described below preclude the use of any other name-value pair for the same Port assignment (i.e., for the same Port number).	Comment by Mirmak, Michael: See Diff_port and Reference below, however...

Diff_port:	The Diff_port value identifies the given Port as one-half of a differential pair and defines the Port number of the complementary port.  Polarity is not directly indicated, since that will be established by how the ports are used in simulation.  Each port declared as a Diff_port shall have a corresponding (complementary) Diff_port declaration.  Note that Diff_port is primarily used for data visualization where, for example, plotting of differential or mixed-mode data for direct, convenient comparison against an industry specification may be automatically performed by an EDA tool.  The Diff_port value refers to the port as a whole.	Comment by Mirmak, Michael: Does this assume that, for instance, DQS_P and DQS_N would be Logical (because these are declarations of function and not of EM polarity)?

Logical:	The Logical value identifies how the Touchstone ports may be used in a schematic symbol, to imply a specific function or usage across different contexts.  For example, a bipolar junction transistor terminal may use the Logical value “emitter” to identify the usage or behavior of the terminal; this is distinct from Physical values (e.g., “B1”), which may have no relation to the functionality of the specific terminal.  Note that connectivity between components in larger structures (e.g., a simulation netlist) is not defined by Logical values.  The Logical name-value pair refers to an individual terminal of the associated Port and is expected to be used primarily as a label. 

Net:		The Net value identifies a collection of terminals for generation of simulation or schematic topologies.  All ports that have the same Net value are part of the same electrical signal path (this does not mean they share the same terminal, as in a short).  Net value identifiers and Physical value identifiers (described below) are the primary mechanisms by which connectivity information between the ports of a Touchstone data set used as a model and its surroundings (e.g., other Touchstone files, SPICE component descriptions, IBIS packages, etc.) may be provided.  Nevertheless, Touchstone files do not name the IBIS-related files, SPICE netlists, etc. that describe the components to which the ports of the Touchstone data set may be connected.  Instead, the connectivity is defined in the external calling file (e.g., the SPICE netlist, the [Interconnect Model] keyword of an IBIS file, the [EMD Model] keyword of an EMD file, the Ts4file parameter in an AMI file, etc.) that instantiates the Touchstone file with its appropriate syntax.  The information contained in the Touchstone port mapping section facilitates automated generation of such connectivity syntax in the calling files, and/or checking the consistency between the Touchstone file and calling files.  The Net name-value pair refers to an individual terminal of the associated Port.	Comment by Wolff, Randy (DI SW EDA EBS PST AV): “in the .ibs, .emd, .ami, or ?? (for PI) file”	Comment by Mirmak, Michael: Not an exhaustive list of extensions; need to mention wrapper files, netlists, etc.

Physical:	The value for the name “Physical” is a string that describes the physical location of a terminal (and optionally its reference) for use in connection to other devices, circuit elements, etc.  This is at minimum a pin name for a component (such as “B1” on a connector).  The string should clearly indicate where, for instance, the terminal on the described circuit element is to be connected to other terminals in a circuit simulator netlist.  The value following the Physical name is not intended to identify the function of the terminal (the “Logical” name is intended for use in associating terminals with functional labels).  A Physical name-value pair refers to an individual terminal of the associated Port.  

For a Touchstone file which describes a printed circuit board (PCB) system, a C_comp Model or a device package, the value argument to a “Physical” name shall should be a reference designator (also called a “refdes”), followed by a dot and a pin number (e.g., U7.3).  Because there is no explicit identification of PCB systems or device packages that can be automatically read, the usage of reference designator syntax is a recommendation to the model maker.

Physical power, ground, and  reference terminals used in Type P ports may also be grouped collected into groups using the string “Group” (see below).

The rules defined below can be followed to automatically connect the circuit described by the Touchstone network data using Physical name-value pairs to external IBIS [Interconnect Model]s, IBIS [EMD Model]s, IBIS [C Comp Model]s, IBIS AMI Ts4file analog circuits, and IBIS-defined PI models.  The value provided in the various <name>, <pin_name>, and <designator> fields shown below shall match the value used in the IBIS or EMD file referencing this Touchstone file.  For this reason, if Data_usage is present for a given Port Map, a Physical name-value pair shall be present for all Ports in that Port Map. 	Comment by Wolff, Randy (DI SW EDA EBS PST AV): “IBIS [Interconnect Model]s, IBIS [EMD Model]s, IBIS [C Comp Model]s, IBIS-AMI Ts4file analog circuits, and IBIS-defined PI models.”  Last part on PI is up in the air. 

Physical value identifiers and Net value identifiers (described above) are the primary mechanisms by which connectivity information between the ports of a Touchstone data set used as a model and its surroundings (e.g., other Touchstone files, SPICE component descriptions, IBIS packages, etc.) may be provided.  Nevertheless, Touchstone files do not name the IBIS-related files, SPICE netlists, etc. that describe the components to which the ports of the Touchstone data set may be connected.  Instead, the connectivity is defined in the external calling file (e.g., the SPICE netlist, the [Interconnect Model] keyword of an IBIS file, the [EMD Model] keyword of an EMD file, the Ts4file parameter in an AMI file, etc.) that instantiates the Touchstone file with its appropriate syntax.  The information contained in the Touchstone port mapping section facilitates automated generation of such connectivity syntax in the calling files, and/or checking the consistency between the Touchstone file and calling files.	Comment by Mirmak, Michael: This is the most important line to agree on - is connectivity for EMD, etc. ONLY determined by Physical?  Or should Logical be involved?	Comment by Wolff, Randy (DI SW EDA EBS PST AV): “in the .ibs, .emd, .ami, or ?? (for PI) file”	Comment by Mirmak, Michael: Not an exhaustive list of extensions; need to mention wrapper files, netlists, etc.

Allowed Physical names for Data_usage “C_comp_model”:	Comment by Author: Allowed arguments to Physical	Comment by Author: Randy: Ext_Ref may be missing; C_comp_model defines this.  Also noted A_GND is a C_comp_model connection.  
· Buffer_I/O (this is required for C_comp_model)
· Buffer_I
· Pullup_ref
· Pulldown_ref
· Power_clamp_ref
· Gnd_clamp_ref
· Ext_ref

Rules for Data_usage “EMD”:
For Type S Ports, the Physical name shall follow one of the structures listed below:
· an EMD <pin_name> 	Comment by Mirmak, Michael: Per Arpad, does this require < > ?
· <designator>.<pin_name>

For Type P Ports, the Physical name shall follow one of the structures listed below: 
· an EMD <pin_name>	Comment by Mirmak, Michael: Per Arpad, does this require < > ?
· <designator>.<pin_name> 
· Bus_label.<name> 	Comment by Mirmak, Michael: Per Arpad, does this require < > ?
· Group.<name> 
· Bus_label.<designator>.<name> 
· Group.<designator>.<name>

Rules for Data_usage “IBIS_Interconnect”:
For Type S Ports, the Physical name shall follow one of the structures listed below:
· pin.<pin_name>
· pad.<pin_name> 	Comment by Author: Actual usage would be pin.A3, pad.A3, etc.	Comment by Author: Also, .Bus_label is a literal, Group is a literal, but <name> is not.
· buf.<pin_name>

For Type P Ports, the Physical name shall be either pin.<pin_name> or pad.<pin_name>.  The list of Bus_label pins can be determined from the associated .ibs file.  Rail connections to the buffer shall be in one of the following formats:	Comment by Mirmak, Michael: Per Arpad, is Bus_Label needed here?
· Pullup_ref.<pin_name>
· Pulldown_ref.<pin_name>	Comment by Author: <pin_name> to show optionality
· Power_clamp_ref.<pin_name>
·   Gnd_clamp_ref.<pin_name>
· Pullup_ref.Bus_label:<name>
· Pulldown_ref.Bus_label:<name>
· Power_clamp_ref.Bus_label:<name>
·   Gnd_clamp_ref.Bus_label:<name>
· Pullup_ref.Group:<name>
· Pulldown_ref.Group:<name>
· Power_clamp_ref.Group:<name>
· Gnd_clamp_ref.Group:<name>
· Ext_ref 
·   A_gnd

Rules for Data_usage “Ts4file”:
Files identified as Data_usage “Ts4file” shall contain no more and no fewer than four (4) ports.  The usage and connectivity are defined by Ts4file parameters in the calling IBIS .ami file.  No terminal identified with “-“ is permitted for a file identified as Data_usage “Ts4file”.  By IBIS rules, Ts4file references are assumed to be A_gnd.  Group is prohibited for Ts4file.	Comment by Mirmak, Michael: Net makes a difference; don’t want to define Physical allowed names.  Suggested labels: buff_p, buff_n, pad_p, pad_n.  

Probe:	The Probe value identifies the location of the terminal where the Port data is captured, either through simulation or lab measurement.  Specifically, this is a set of coordinates identifying the terminal location.  The value argument to the “Probe” name shall be an X:Y:Z string, with each value,  representing a coordinate, separated from other coordinates by the colon (“:”) character.  Whitespace separating the coordinate values and the colon character is permitted.  X and Y values shall be numeric (floating point) values and are assumed to define distances.  Because PCB system descriptions in Touchstone files may involve either a physical distance (e.g., the top of a connector on a PCB) Z may be a numeric (floating point) value to describe a distance, or to describe a layer within a PCB stackup, the Z value may be a non-negative integer or a string without whitespace.  The coordinate origin is arbitrary and not stated in the Touchstone file, but all coordinates used in a single Touchstone file port map shall use the same origin.  Note that Probe values may refer to a measurement fixture or system not described in the Touchstone file data.  This fixture or system may be distinct from any terminal information in Net and/or Physical used for connectivity to other components.

Probe coordinate values have no meaning for the purposes of connectivity, unlike Net and Physical values.  

Side:	The Side value identifies a collection of ports, to help define a functional orientation of the ports relative to other ports on the same component; this is a way to collect Logical functions according to Physical associations.  Interconnects described by Touchstone often have two sides; for instance, a connector linking a mainboard and daughterboard.  Ports on such a connector may therefore have Side values of “mainboard” and “daughterboard”.  A memory DQ route may have a Controller Side, and separate Sides for each memory device connected to that route.  Similarly, a cable assembly for a car may have four Sides (e.g., CPU, Brake, Engine, and Camera).  Note that, like Logical values, values used with Side should not be used for establishing or cross-checking physical connectivity; the Side value is primarily intended as a label.  The Side value refers to the port as a whole.

Type:	The value following the name “Type” shall be either the S or the P character.  S stands for Signal, while P stands for Power (in other words, rail).  If not specified, the Type default is S.  The Type name-value pair refers to the port as a whole.	Comment by Mirmak, Michael: Does this mean that Type really refers to the + and not the - or Reference?  The - could be a Rail, after all.

UD: 	For UD data on Port lines, the data shall follow the string UD and whitespace within the same pair of parentheses.  UD information effectively will be ignored by EDA tools, but may be used to track how the data describing the port behavior was generated, and/or how the Port data was physically measured.

Name-value pairs for Logical, Net, Physical, or Probe preceded with a “-“ character define how the reference terminal for that function of the port is connected, or the reference terminal used for measurement for that function.  The value in these reference terminal name-value pairs may be different for each port or may be the same for some ports (in any combination) or may be the same for all ports.  A_gnd may be used as the reference terminal of some or all ports.  Using A_gnd in a name-value pair identified with “-“ is equivalent to omitting that name-value pair since A_gnd is the assumed (or default) reference connection.  This notation helps model makers document how the probes or ports were set up in the lab measurements or extraction software simulations.  Note that the use of A_gnd for Logical name-value references does not have meaning in terms of  connectivity, measurement, or defining a return path; it is simply a label.  Similarly, for Probe, the use of A_gnd does not have meaning in terms of connectivity or defining a return path; the “A_gnd” string for Probe, if present, simply names a common reference used for measurement of the provided data without specifying a precise physical location.
How referencing is handled when the Touchstone data is used in simulation is entirely up to the user of the data or the EDA simulation software.  Care must be taken to ensure that Touchstone data used as models and other circuit blocks (if present) are connected without compromising the loop behavior of the overall circuit being simulated.

Physical rail-connected terminals (Type P) may be collected into Groups.  Here, the string “Group” precedes a string identifier as part of a Physical name-value pair on the Port line (this includes Physical name-value pairs preceded by “-“).  A matching string identifier shall appear as part of the Group subparameter after the Port lines.  Note that Group is not supported for name-value types other than Physical.

Diff_port does not identify polarity; it may be declared for a Port where the “-“ symbol is used.  There is no conflict using both syntax features, as Diff_port is intended for use in visualization of data.  EDA tools are responsible for providing clear controls to users regarding connectivity and data display when Diff_port and the “-“ symbol are present for the same Port(s).  Finally, Diff_port is not a declaration that mixed-mode data is present.  	Comment by Mirmak, Michael: Both terminals in the same Diff_port declaration have the same reference.	Comment by Mirmak, Michael: Add note regarding all data being single-ended; Diff_port is not a declaration that mixed-mode data is present.

The asterisk character (“*”) may be used as a wildcard for Data_usage EMD to represent multiple terminals, but only in the context of references (meaning, with a name-value pair and the “-“ symbol), ports identified as “Type P” (meaning, where power rails are involved), or where the Group parameter is used.

In the absence of wildcards, the number of terminals for a given structure may be calculated based on the number of unique Physical and/or Logical name-value pairs present.


Example 1:   5 signals of a cable connected from a CPU to a sensor.

| Each of these ports uses A_gnd as a reference as no “-“ terminals
| are declared.
[Begin Port Map] 
Port 1 (Physical A.1)(Side CPU)(Net 1)
Port 2 (Physical A.2)(Side CPU)(Net 2)
Port 3 (Physical A.3)(Side CPU)(Net 3)
Port 4 (Physical A.4)(Side CPU)(Net 4)
Port 5 (Physical A.5)(Side CPU)(Net 5)
Port 6 (Physical B.1)(Side Sensor)(Net 1)
Port 7 (Physical B.2)(Side Sensor)(Net 2)
Port 8 (Physical B.3)(Side Sensor)(Net 3)
Port 9 (Physical B.4)(Side Sensor)(Net 4)
Port 10 (Physical B.5)(Side Sensor)(Net 5)

Symbol_leftside 1 2 3 4 5
Symbol_rightside 6 7 8 9 10
[End Port Map]

Example 2a:   Description of the measurement of a bipolar junction transistor, common emitter.	Comment by Mirmak, Michael: Suggest making this discouraged or illegal without Physical declaration; should Physical be required?

| Note that this describes how a set of S-parameters were collected to characterize a 
| device for use in RF applications.  The name-value pairs establish this as a 2-port, 
| 3-terminal device.
[Begin Port Map] 
Port 1 ( Logical Base )      -( Logical Emitter ) ( Probe 32.5:16.0:6.0 )  -( Probe 7.0:10.0:2.0 )
Port 2 ( Logical Collector ) -( Logical Emitter ) ( Probe 29.5:13.0:3.0 )  -( Probe 7.0:10.0:2.0 )
[End Port Map]


Example 2b:   Description of the measurement of a bipolar junction transistor, common collector.	Comment by Mirmak, Michael: Suggest making this discouraged or illegal without Physical declaration; should Physical be required?

| Note that this describes how a set of S-parameters were collected to characterize a 
| device for use in RF applications.  The name-value pairs used establish this as a 
| 2-port, 3-terminal device.
[Begin Port Map] 
Port 1 ( Logical Base )    -( Logical Collector ) (Probe 32.5:16.0:6.0) –( Probe 29.5:13.0:3.0)
Port 2 ( Logical Emitter ) -( Logical Collector ) (Probe 7.0:10.0:2.0) –( Probe 29.5:13.0:3.0)
[End Port Map]


Example 2c:   Description of the measurement of a bipolar junction transistor, common collector.	Comment by Mirmak, Michael: Suggest making this discouraged or illegal without Physical declaration; should Physical be required?

| Note that this describes how a set of S-parameters were collected to characterize a 
| device for use in RF applications.  The name-value pairs used establish this as a 
| 2-port, 3-terminal device.
[Begin Port Map] 
Port 1 ( Logical Collector ) -( Logical Base ) (Probe 29.5:13.0:3.0)  –(Probe 32.5:16.0:6.0
Port 2 ( Logical Emitter )   -( Logical Base ) (Probe 7.0:10.0:2.0) –(Probe 32.5:16.0:6.0)
[End Port Map]


Example 2d:   Measurement data for a bipolar junction transistor with single reference

| Here, all three terminals are represented using ports with respect to a separate 
| reference.  Note that the reference terminal may be omitted; in that case, A_gnd would 
| be assumed.  The [Number of Ports] field is 3 and the number of terminals is 4.
[Begin Port Map] 
Port 1 (Physical 1) (Logical Base)      -(Physical probe_ref) (Side B) (Probe 32.5:16.0:6.0) –(Probe 10.0:20.5:1)        
Port 2 (Physical 2) (Logical Collector) –(Physical probe_ref) (Side C) (Probe 29.5:13.0:3.0) –(Probe 10.0:20.5:1)
Port 3 (Physical 3) (Logical Emitter)   -(Physical probe_ref) (Side E) (Probe 7.0:10.0:2.0) –(Probe 10.0:20.5:1)	Comment by Mirmak, Michael: Must we have matched +/- for each name-value pair?  In other words, is there a Logical reference here?
[End Port Map]


Example 2e:   Model data for a bipolar junction transistor with symbol information for a schematic.

| Here, all three terminals are represented using ports with respect to the ideal
| reference (A_gnd).  The [Number of Ports] field is 3.  The number of terminals in a 
| symbol could be 3 or 4 depending on connectivity to other components.  The references 
| here are unstated, but default to A_gnd.
[Begin Port Map] 
Port 1 (Logical Base)      (Physical 1) (Probe 32.5:16.0:6.0)
Port 2 (Logical Collector) (Physical 2) (Probe 29.5:13.0:3.0)
Port 3 (Logical Emitter)   (Physical 3) (Probe 7.0:10.0:2.0)
[End Port Map]


Example 192f: Independent references in a set of transistor measurements, with user-defined data after Port definitions.

| Here, all three terminals are represented using ports with respect to a separate 
| reference.  Note that the reference terminal may be omitted; in that case, A_gnd would 
| be assumed.  The [Number of Ports] field is 3 and the number of terminals is 4.
[Begin Port Map] 
Port 1 ( Physical 1 ) ( Logical Base )      -( Physical probe_ref ) (Side B)         (Probe 32.5:16.0:6.0) –(Probe 0.0:20.5:1)
Port 2 ( Physical 2 ) ( Logical Collector ) –( Physical probe_ref ) (Side C) (Probe 29.5:13.0:3.0) –(Probe 0.0:20.5:1)
Port 3 ( Physical 3 ) ( Logical Emitter )   -( Physical probe_ref ) (Side E) (Probe 7.0:10.0:2.0) –(Probe 0.0:20.5:1)	Comment by Mirmak, Michael: Must we have matched +/- for each name-value pair?  In other words, is there a Logical reference here?
UD SijStatus 1 2 Measured	
[End Port Map]


Example 20g: Independent references in a set of transistor measurements, with user-defined data identified in-line with the Port definitions.

| Here, all three terminals are represented using ports with respect to a separate 
| reference.  Note that the reference terminal may be omitted; in that case, A_gnd would 
| be assumed.  The [Number of Ports] field is 3 and the number of terminals is 4.
[Begin Port Map] 
Port 1 (Physical 1)(Logical Base) -(Physical probe_ref)(Side B) (Probe 32.5:16.0:6.0) –(Probe 0.0:20.5:1) (UD SijStatus Measured)
Port 2 (Physical 2)(Logical Collector) –(Physical probe_ref)(Side C) (Probe 29.5:13.0:3.0) –(Probe 0.0:20.5:1) (UD SijStatus Measured)
Port 3 (Physical 3)(Logical Emitter)  -(Physical probe_ref)(Side E) (Probe 7.0:10.0:2.0) –(Probe 0.0:20.5:1)	Comment by Mirmak, Michael: Must we have matched +/- for each name-value pair?  In other words, is there a Logical reference here?
[End Port Map]


Example 3a:   An 8” coplanar wave guide (3 connections: 1 signal and 2 references).

[Begin Port Map] 
Port 1 ( Physical pin.A3 ) (Net 1) (Side Left)  -( Physical pin.H7 )
Port 2 ( Physical pin.A4 ) (Net 1) (Side Right) -( Physical Group:GND_R )	Comment by Mirmak, Michael: As above, should Net have a reference here?	Comment by Mirmak, Michael: | This assumes system usage information, even if A3, A4, H7 and GND_R are defined only 
| for this component?
| H7 is NOT part of a Port; nor is GND_R (both correctly).  Does this mean that the SPICE circuit for this component has four terminals?   
Group Physical GND_R (pin.C6 pin.D8)
[End Port Map]


Example 3b:   An 8” coplanar wave guide (probe has 3 connections: 1 signal and 2 references).

[Begin Port Map] 
Port 1 (Physical pin.A3) (Net 1) (Side Left)  -( Physical Group:GND_L )	Comment by Wolff, Randy (DI SW EDA EBS PST AV): Ports are duplicated. Looks like first two Port lines should be removed based on inclusion of Group references.
Port 2 (Physical pin.A4) (Net 1) (Side Right) –( Physical Group:GND_R )
Group Physical GND_L (pin.E7 pin.F8)	Comment by Mirmak, Michael: | GND_L and GND_R are NOT part of any Ports (correctly).  Does this mean that the SPICE circuit for this component has four terminals?
Group Physical GND_R (pin.C6 pin.D8)	Comment by Mirmak, Michael: | This assumes system usage information, even if A3, A4, H7 and GND_R are defined only 
| for this component?
[End Port Map]


Example 4:  Single-ended IBIS package [Interconnect Model] between pin and pad on pin 7.

| IBIS Interconnect does not currently support documentation of per-port 
| references
[Begin Port Map] 
Data_usage "IBIS_Interconnect"
Port 1 (Physical pin.7) (Net 7) (Logical DQ3pin) –(pin.8) (Side Pin)	Comment by Wolff, Randy (DI SW EDA EBS PST AV): Maybe add “(Reference pad.8)” for local pad reference
Port 2 (Physical pad.7) (Net 7) (Logical DQ3pad) –(pad.8) (Side Pad)	Comment by Wolff, Randy (DI SW EDA EBS PST AV): Maybe add “(Reference pad.8)” for local pad reference
[End Port Map]


Example 5:  Single-ended IBIS package [Interconnect Model] between pin and buffer on pin 7, including VDD voltage port.  Not sure about this example, since the IBIS Vss pin is theoretically “floating” this way.  I don’t want to encourage people to do bad things with this example…

[Begin Port Map] 
Data_usage "IBIS_Interconnect"
Port 1 (Physical pin.7) (Type S) (Side Pin)   (Net 7) (Logical DQ3pin)  
| Type S is redundant, as this is the default
Port 2 (Physical buf.7) (Type S) (Side Buffer)(Net 7) (Logical DQ3buffer) 
| Type S is redundant, as this is the default
Port 3 (Physical Pin.Bus_label:VDD)(Type P)(Side Pin)   (Net VDD)(Logical VDDpin)
Port 4 (Physical Pullup_ref.7)     (Type P)(Side Buffer)(Net VDD)(Logical VDDbuffer)
[End Port Map]


Example 6:  Single-ended connection between components U1.7 and U3.5 on a PCB.	Comment by Wolff, Randy (DI SW EDA EBS PST AV): Does this example add any value? 
	Comment by Mirmak, Michael: | This assumes system usage information due to Physical declarations, but also carries Logical
| information. 
| Critical question: are U1 and U3 reference designators in the full system? Or just for this part?
| The lack of “Data_usage” implies that these are “local” only.
[Begin Port Map] 
Port 1 (Physical U1.7)(Side U1)(Net DQ3)(Logical CPU)
Port 2 (Physical U3.5)(Side U3)(Net DQ3)(Logical SDRAM)
[End Port Map]


Example 7:  IBIS [EMD Model] of a 4-bit DQ nibble in a 2-rank DIMM.	Comment by Wolff, Randy (DI SW EDA EBS PST AV): Mem1/mem2 sides updated to use reference designator pins instead of EMD pins

[Begin Port Map] 	Comment by Mirmak, Michael: | This assumes system usage information due to Physical declarations, but also carries Logical
| information.
| Critical question: are U1 and U2 reference designators in the full system?  Or just for this part?
| The presence of “Data _usage” implies that these are full system identifiers.
Data_usage "EMD"
Port 1 (Physical  20)   (Side EMD) (Net DQ0) (Logical DQ0)
Port 2 (Physical  21)   (Side EMD) (Net DQ1) (Logical DQ1)
Port 3 (Physical  22)   (Side EMD) (Net DQ2) (Logical DQ2)
Port 4 (Physical  23)   (Side EMD) (Net DQ3) (Logical DQ3)
Port 5 (Physical  24)   (Side EMD) (Net DQS+)(Logical DQS+)      (Diff_port 6)
Port 6 (Physical  25)   (Side EMD) (Net DQS-)(Logical DQS-)      (Diff_port 5)
Port 7 (Physical  U1.A2)(Side mem1)(Net DQ0) (Logical mem1_DQ0)
Port 8 (Physical  U1.A3)(Side mem1)(Net DQ1) (Logical mem1_DQ1)
Port 9 (Physical  U1.B2)(Side mem1)(Net DQ2) (Logical mem1_DQ2)
Port 10 (Physical U1.B3)(Side mem1)(Net DQ3) (Logical mem1_DQ3)
Port 11 (Physical U1.A4)(Side mem1)(Net DQS+)(Logical mem1_DQS+) (Diff_port 12)
Port 12 (Physical U1.B4)(Side mem1)(Net DQS-)(Logical mem1_DQS-) (Diff_port 11)
Port 13 (Physical U2.A2)(Side mem2)(Net DQ0) (Logical mem2_DQ0)
Port 14 (Physical U2.A3)(Side mem2)(Net DQ1) (Logical mem2_DQ1)
Port 15 (Physical U2.B2)(Side mem2)(Net DQ2) (Logical mem2_DQ2)
Port 16 (Physical U2.B3)(Side mem2)(Net DQ3) (Logical mem2_DQ3)
Port 17 (Physical U2.A4)(Side mem2)(Net DQS+)(Logical mem2_DQS+) (Diff_port 18)
Port 18 (Physical U2.B4)(Side mem2)(Net DQS-)(Logical mem2_DQS-) (Diff_port 17)
| The parameters below will generate a symbol
| where DQS+ and DQS- are presented at the top of the left and right
| sides of the symbol
Symbol_leftside  5, 6, 1, 2, 3, 4
Symbol_rightside 11, 12, 7, 8, 9, 10, 17, 18, 13, 14, 15, 16
[End Port Map]	
[image: ]Figure 1 - Dual-Rank DIMM with EMD



Example 8:  4-port Touchstone file for a differential buffer.	Comment by Wolff, Randy (DI SW EDA EBS PST AV): Remove this example.  Repeat of Example 1, and IBIS_file has been removed.

[Begin Port Map]	Comment by Mirmak, Michael: | This assumes system usage information due to Physical declarations. 
| Critical question: are A and B reference designators in the full system? Or just for this part? 
| Implied to be the latter, but we have no way to distinguish between this case and Examples 6 and 
| 7 beyond “Data_usage”.
Data_usage "Ts4file"
Port 1 (Physical A.1)  (Side Die) (Net 1) (Diff_port 2)
Port 2 (Physical A.2)  (Side Die) (Net 2) (Diff_port 1)
Port 3 (Physical B.1)  (Side Pin) (Net 1) (Diff_port 4)
Port 4 (Physical B.2)  (Side Pin) (Net 2) (Diff_port 3)
[End Port Map]


Example 9:  C_comp Model for an input buffer IBIS model.	Comment by Wolff, Randy (DI SW EDA EBS PST AV): Remove this example.  Repeat of Example 1, and IBIS_file has been removed.

[Begin Port Map]
Data_usage "C_comp_model"
Port 1 (Type S) (Physical Buffer_I)   
Port 2 (Type S) (Physical Buffer_I/O)
| Buffer_I/O is required for all C_comp_models
| A_gnd is the default reference
[End Port Map]


Example 10: An EMD-like model example with “per interface” referencing using Group (this approach is not currently supported by EMD in IBIS through version 8.0, as EMD permits only one reference connection for all ports).

[Begin Port Map]
Port 1  (Type S) (Side Die1)  (Physical U1.94)(Net A0) –( Physical Group:GND_U1 )
Port 2  (Type S) (Side Die2)  (Physical U2.94)(Net A0) –( Physical Group:GND_U2 )
Port 3  (Type S) (Side Die3)  (Physical U3.94)(Net A0) –( Physical Group:GND_U3 )
Port 4  (Type S) (Side EMDpin)(Physical K2)   (Net A0) –( Physical Group:GND_BGA )
…
Port 7  (Type S) (Physical U1.95)(Side Die1)  (Net A1) –( Physical Group:GND_U1 )
Port 8  (Type S) (Physical U2.95)(Side Die2)  (Net A1) –( Physical Group:GND_U2 )
Port 9  (Type S) (Physical U3.95)(Side Die3)  (Net A1) –( Physical Group:GND_U3 )
Port 10 (Type S) (Physical J2)   (Side EMDpin)(Net A1) –( Physical Group:GND_BGA )
…
Port 121 (Type S)(Side Die1)  (Physical U1.71)(Net CLK_c) –(Physical Group:GND_U1) (Diff_port 123)
Port 122 (Type S)(Side EMDpin)(Physical E2)   (Net CLK_c) -(Physical Group:GND_BGA)(Diff_port 124)
Port 123 (Type S)(Side Die1)  (Physical U1.70)(Net CLK_t) –(Physical Group:GND_U1) (Diff_port 121)
Port 124 (Type S)(Side EMDpin)(Physical D2)   (Net CLK_t) -(Physical Group:GND_BGA)(Diff_port 122)
…
Port 163 (Type P) (Physical Group:VDD_U1)  (Net VDD) (Side Die1)   –(Physical Group:GND_U1)
Port 164 (Type P) (Physical Group:VDD_U2)  (Net VDD) (Side Die2)   –(Physical Group:GND_U2)
Port 165 (Type P) (Physical Group:VDD_U3)  (Net VDD) (Side Die3)   –(Physical Group:GND_U3)
Port 166 (Type P) (Physical Group:VDD_BGA) (Net VDD) (Side EMDpin) –(Physical Group:GND_BGA)
…
Group Physical VDD_U1 (U1.4 U1.8 U1.17 U1.20 U1.33 U1.36 U1.40 U1.45 U1.49 U1.52 ...)
Group Physical VDD_U2 (U2.4 U2.8 U2.17 U2.20 U2.33 U2.36 U2.40 U2.45 U2.49 U2.52 ...)
Group Physical VDD_U3 (U3.4 U3.8 U3.17 U3.20 U3.33 U3.36 U3.40 U3.45 U3.49 U3.52 ...)
Group Physical VDD_BGA (BGA.A3 BGA.A4 BGA.A7 BGA.AB5 BGA.AB9 BGA.AB11 BGA.B1 BGA.B5...)
…
Group Physical GND_U1 (U1.2 U1.11 U1.15 U1.23 U1.38 U1.42 U1.43 U1.47 U1.50 U1.54 ...)
Group Physical GND_U2 (U2.2 U2.11 U2.15 U2.23 U2.38 U2.42 U2.43 U2.47 U2.50 U2.54 ...)
Group Physical GND_U3 (U3.2 U3.11 U3.15 U3.23 U3.38 U3.42 U3.43 U3.47 U3.50 U3.54 ...)
Group Physical GND_BGA (BGA.A5 BGA.A9 BGA.A11 BGA.A14 BGA.AA5 BGA.AA13 BGA.AC14...)
[End Port Map]


Example 11: An EMD-like model example with one reference at all Designator pins and another at EMD pins using Group with RefDes wildcards (this approach is not currently supported by EMD in IBIS through version 8.0, as EMD permits only one reference connection for all ports).	Comment by Author: We may need to invent support for wildcards

[Begin Port Map]
Port 1   (Type S) (Physical U1.94) (Net A0) (Side Die1)   –(Physical Group:GND_Ux)
Port 2   (Type S) (Physical U2.94) (Net A0) (Side Die2)   –(Physical Group:GND_Ux)
Port 3   (Type S) (Physical U3.94) (Net A0) (Side Die3)   –(Physical Group:GND_Ux)
Port 4   (Type S) (Physical K2)    (Net A0) (Side EMDpin) –(Physical Group:GND_BGA)
…
Port 7   (Type S) (Physical U1.95) (Net A1) (Side Die1)   –(Physical Group:GND_Ux)
Port 8   (Type S) (Physical U2.95) (Net A1) (Side Die2)   –(Physical Group:GND_Ux)
Port 9   (Type S) (Physical U3.95) (Net A1) (Side Die3)   –(Physical Group:GND_Ux)
Port 10  (Type S) (Physical J2)    (Net A1) (Side EMDpin) –(Physical Group:GND_BGA)
…
Port 121 (Type S)(Side Die1)  (Physical U1.71)(Net CLK_c) –(Physical Group:GND_Ux) (Diff_port 123)
Port 122 (Type S)(Side EMDpin)(Physical E2)   (Net CLK_c) –(Physical Group:GND_BGA)(Diff_port 124)
Port 123 (Type S)(Side Die1)  (Physical U1.70)(Net CLK_t) –(Physical Group:GND_Ux) (Diff_port 121)
Port 124 (Type S)(Side EMDpin)(Physical D2)   (Net CLK_t) -(Physical Group:GND_BGA)(Diff_port 122)
…
Port 163 (Type P) (Side Die1)  (Physical Group:VDD_U1)  (Net VDD) –(Physical Group:GND_Ux)
Port 164 (Type P) (Side Die2)  (Physical Group:VDD_U2)  (Net VDD) –(Physical Group:GND_Ux)
Port 165 (Type P) (Side Die3)  (Physical Group:VDD_U3)  (Net VDD) –(Physical Group:GND_Ux)
Port 166 (Type P) (Side EMDpin)(Physical Group:VDD_BGA) (Net VDD) –(Physical Group:GND_BGA)
…
Group Physical VDD_U1  (U1.4  U1.8  U1.17  U1.20  U1.33  U1.36  U1.40   U1.45   U1.49  U1.52 ...)
Group Physical VDD_U2  (U2.4  U2.8  U2.17  U2.20  U2.33  U2.36  U2.40   U2.45   U2.49  U2.52 ...)
Group Physical VDD_U3 (U3.4  U3.8  U3.17  U3.20  U3.33  U3.36  U3.40   U3.45   U3.49  U3.52 ...)

Group Physical VDD_BGA (BGA.A3 BGA.A4 BGA.A7 BGA.AB5 BGA.AB9 BGA.AB11 BGA.AB13 BGA.AC7 BGA.B1 BGA.B5...)
…
Group Physical GND_Ux  (*.2    *.11   *.15    *.23    *.38    *.42     *.43    *.47    *.50     *.54 ...)
Group Physical GND_BGA (BGA.A5 BGA.A9 BGA.A11 BGA.A14 BGA.AA5 BGA.AA13 BGA.AC5 BGA.AC9 BGA.AC11 BGA.AC14...)
[End Port Map]


[bookmark: _Hlk209012836]Example 12: An EMD-like model example with “per interface” referencing using EMD rail signal names (this approach is not currently supported by EMD in IBIS through version 8.0, as EMD permits only one reference connection for all ports).	Comment by Author: How do we know these are rail signal names?

[Begin Port Map]
Port 1   (Type S) (Side Die1)  (Physical U1.94) (Net A0) -(Physical U1.GND)
Port 2   (Type S) (Side Die2)  (Physical U2.94) (Net A0) -(Physical U2.GND)
Port 3   (Type S) (Side Die3)  (Physical U3.94) (Net A0) -(Physical U3.GND)
Port 4   (Type S) (Side EMDpin)(Physical K2)    (Net A0) -(Physical GND)
…
Port 7   (Type S) (Side Die1)   (Physical U1.95) (Net A1) -(Physical U1.GND)
Port 8   (Type S) (Side Die2)   (Physical U2.95) (Net A1) -(Physical U2.GND)
Port 9   (Type S) (Side Die3)   (Physical U3.95) (Net A1) -(Physical U3.GND)
Port 10  (Type S) (Side EMDpin) (Physical J2)    (Net A1) –(Physical GND)
…
Port 121 (Type S)(Side Die1)  (Physical U1.71)(Net CLK_c) -(Physical U1.GND)(Diff_port 123)
Port 122 (Type S)(Side EMDpin)(Physical E2)   (Net CLK_c) –(Physical GND)   (Diff_port 124)
Port 123 (Type S)(Side Die1)  (Physical U1.70)(Net CLK_t) -(Physical U1.GND)(Diff_port 121)
Port 124 (Type S)(Side EMDpin)(Physical D2)   (Net CLK_t) –(Physical GND)   (Diff_port 122)
…
Port 163 (Type P) (Side Die1)   (Physical U1.VDD) (Net VDD) -(Physical U1.GND)
Port 164 (Type P) (Side Die2)   (Physical U2.VDD) (Net VDD) -(Physical U2.GND)
Port 165 (Type P) (Side Die3)   (Physical U3.VDD) (Net VDD) -(Physical U3.GND)
Port 166 (Type P) (Side EMDpin) (Physical VDD)    (Net VDD) –(Physical GND)
[End Port Map]


Example 13: An EMD-like model example with one reference at all Designator pins and another at EMD pins using EMD rail signal names with RefDes wildcards (this approach is not currently supported by EMD in IBIS through version 8.0, as EMD permits only one reference connection for all ports).	Comment by Author: How do we know these are rail signal names?	Comment by Author: We may need to invent support for wildcards

[Begin Port Map]
Port 1   (Type S) (Side Die1)   (Physical U1.94) (Net A0) -(Physical *.GND )
Port 2   (Type S) (Side Die2)   (Physical U2.94) (Net A0) -(Physical *.GND )
Port 3   (Type S) (Side Die3)   (Physical U3.94) (Net A0) -(Physical *.GND )
Port 4   (Type S) (Side EMDpin) (Physical K2)    (Net A0) –(Physical GND )
…
Port 7   (Type S) (Side Die1)   (Physical U1.95) (Net A1) -(Physical *.GND )
Port 8   (Type S) (Side Die2)   (Physical U2.95) (Net A1) -(Physical *.GND )
Port 9   (Type S) (Side Die3)   (Physical U3.95) (Net A1) -(Physical *.GND )
Port 10  (Type S) (Side EMDpin) (Physical J2)    (Net A1) –(Physical GND )
…
Port 121 (Type S)(Side Die1)  (Physical U1.71)(Net CLK_c) -(Physical *.GND)(Diff_port 123)
Port 122 (Type S)(Side EMDpin)(Physical E2)   (Net CLK_c) –(Physical GND)  (Diff_port 124)
Port 123 (Type S)(Side Die1)  (Physical U1.70)(Net CLK_t) -(Physical *.GND)(Diff_port 121)
Port 124 (Type S)(Side EMDpin)(Physical D2)   (Net CLK_t) –(Physical GND)  (Diff_port 122)
…
Port 163 (Type P) (Physical U1.VDD) (Side Die1)  (Net VDD) -(Physical *.GND )
Port 164 (Type P) (Physical U2.VDD) (Side Die2)  (Net VDD) -(Physical *.GND )
Port 165 (Type P) (Physical U3.VDD) (Side Die3)  (Net VDD) -(Physical *.GND )
Port 166 (Type P) (Physical VDD)    (Side EMDpin)(Net VDD) –(Physical GND )
[End Port Map]


Example 14: An EMD model example with a single reference for all ports using EMD rail signal names (This is currently the referencing method supported by EMD in IBIS through version 8.0.  While legal in EMD files, this approach leaves the Designator ground pins floating.).	Comment by Author: How do we know these are rail signal names?

[Begin Port Map]
Port 1   (Type S) (Side Die1)   (Physical U1.94) (Net A0) –(Physical GND)
Port 2   (Type S) (Side Die2)   (Physical U2.94) (Net A0) –(Physical GND)
Port 3   (Type S) (Side Die3)   (Physical U3.94) (Net A0) -(Physical GND)
Port 4   (Type S) (Side EMDpin) (Physical K2)    (Net A0) -(Physical GND)
…
Port 7   (Type S) (Side Die1)   (Physical U1.95) (Net A1) –(Physical GND)
Port 8   (Type S) (Side Die2)   (Physical U2.95) (Net A1) –(Physical GND)
Port 9   (Type S) (Side Die3)   (Physical U3.95) (Net A1) –(Physical GND)
Port 10  (Type S) (Side EMDpin) (Physical J2)    (Net A1) –(Physical GND)
…
Port 121 (Type S) (Side Die1)   (Physical U1.71) (Net CLK_c) -(Physical GND)(Diff_port 123)
Port 122 (Type S) (Side EMDpin) (Physical E2)    (Net CLK_c) -(Physical GND)(Diff_port 124)
Port 123 (Type S) (Side Die1)   (Physical U1.70) (Net CLK_t) -(Physical GND)(Diff_port 121)
Port 124 (Type S) (Side EMDpin) (Physical D2)    (Net CLK_t) –(Physical GND)(Diff_port 122)
…
Port 163 (Type P) (Side Die1)   (Physical U1.VDD) (Net VDD) –(Physical GND)
Port 164 (Type P) (Side Die2)   (Physical U2.VDD) (Net VDD) –(Physical GND)
Port 165 (Type P) (Side Die3)   (Physical U3.VDD) (Net VDD) –(Physical GND)
Port 166 (Type P) (Side EMDpin) (Physical VDD)    (Net VDD) –(Physical GND)
[End Port Map]


Example 15: An EMD model example with a single reference for all ports using A_gnd (This is currently the referencing method supported by EMD in IBIS through version 8.0.  While legal in EMD files, this approach does not define any EMD or Designator ground pins, leaving the Designator ground pins floating.).	Comment by Author: Do we need to define “A_gnd” as a special word for such uses?

[Begin Port Map]
Port 1   (Type S)(Physical U1.94)(Side Die1)  (Net A0)
Port 2   (Type S)(Physical U2.94)(Side Die2)  (Net A0)
Port 3   (Type S)(Physical U3.94)(Side Die3)  (Net A0)
Port 4   (Type S)(Physical K2)   (Side EMDpin)(Net A0)
…
Port 7   (Type S)(Physical U1.95)(Side Die1)  (Net A1)
Port 8   (Type S)(Physical U2.95)(Side Die2)  (Net A1)
Port 9   (Type S)(Physical U3.95)(Side Die3)  (Net A1)
Port 10  (Type S)(Physical J2)   (Side EMDpin)(Net A1)
…
Port 121 (Type S)(Physical U1.71)(Side Die1)  (Net CLK_c)(Diff_port 123)
Port 122 (Type S)(Physical E2)   (Side EMDpin)(Net CLK_c)(Diff_port 124)
Port 123 (Type S)(Physical U1.70)(Side Die1)  (Net CLK_t)(Diff_port 121)
Port 124 (Type S)(Physical D2)   (Side EMDpin)(Net CLK_t)(Diff_port 122)
…
Port 163 (Type P)(Physical U1.VDD)(Side Die1)  (Net VDD)
Port 164 (Type P)(Physical U2.VDD)(Side Die2)  (Net VDD)
Port 165 (Type P)(Physical U3.VDD)(Side Die3)  (Net VDD)
Port 166 (Type P)(Physical VDD)   (Side EMDpin)(Net VDD)
[End Port Map]


Example 16: An EMD model example with a single reference for all ports using A_gnd and additional ports to connect the EMD and Designator ground pins.  (This is legal in EMD files and provides a complete definition for all EMD and Designator ground pins).	Comment by Author: Do we need to define “A_gnd” as a special word for such uses?

[Begin Port Map]
Data_usage "EMD"
Port 1   (Type S)(Physical U1.94)(Side Die1)  (Net A0)
Port 2   (Type S)(Physical U2.94)(Side Die2)  (Net A0)
Port 3   (Type S)(Physical U3.94)(Side Die3)  (Net A0)
Port 4   (Type S)(Physical K2)   (Side EMDpin)(Net A0)
…
Port 7   (Type S)(Physical U1.95)(Side Die1)  (Net A1)
Port 8   (Type S)(Physical U2.95)(Side Die2)  (Net A1)
Port 9   (Type S)(Physical U3.95)(Side Die3)  (Net A1)
Port 10  (Type S)(Physical J2)   (Side EMDpin)(Net A1)
…
Port 121 (Type S)(Physical U1.71)(Side Die1)  (Net CLK_c)(Diff_port 123)
Port 122 (Type S)(Physical E2)   (Side EMDpin)(Net CLK_c)(Diff_port 124)
Port 123 (Type S)(Physical U1.70)(Side Die1)  (Net CLK_t)(Diff_port 121)
Port 124 (Type S)(Physical D2)   (Side EMDpin)(Net CLK_t)(Diff_port 122)
…
Port 163 (Type P)(Physical U1.VDD)(Side Die1)  (Net VDD)
Port 164 (Type P)(Physical U2.VDD)(Side Die2)  (Net VDD)
Port 165 (Type P)(Physical U3.VDD)(Side Die3)  (Net VDD)
Port 166 (Type P)(Physical VDD)   (Side EMDpin)(Net VDD)
…
Port 200 (Type P)(Physical U1.GND)(Side Die1)  (Net GND)
Port 201 (Type P)(Physical U2.GND)(Side Die2)  (Net GND)
Port 202 (Type P)(Physical U3.GND)(Side Die3)  (Net GND)
Port 203 (Type P)(Physical GND)   (Side EMDpin)(Net GND)
[End Port Map]


Example 17: An IBIS package [Interconnect Model] example with pin rail grouping and using pad names (the model is between pin and pad).	Comment by Author: We may need to invent ways to refer to pad names

[Begin Port Map]
Data_usage "IBIS_Interconnect"
Port 1   (Type S)(Physical A7)(Side Pin_IO)   (Net DM_n)
Port 2   (Type S)(Physical A7)(Side Pad_IO)   (Net DM_n)
Port 3   (Type S)(Physical C2)(Side Pin_IO)   (Net DQ0) 
Port 4   (Type S)(Physical C2)(Side Pad_IO)   (Net DQ0) 
Port 5   (Type S)(Physical B7)(Side Pin_IO)   (Net DQ1) 
Port 6   (Type S)(Physical B7)(Side Pad_IO)   (Net DQ1) 
Port 7   (Type S)(Physical D3)(Side Pin_IO)   (Net DQ2) 
Port 8   (Type S)(Physical D3)(Side Pad_IO)   (Net DQ2)

Port 9   (Type S)(Physical B3)(Side Pin_IO)   (Net DQS_c) (Diff_port 11)
Port 10  (Type S)(Physical B3)(Side Pad_IO)   (Net DQS_c) (Diff_port 12)
Port 11  (Type S)(Physical C3)(Side Pin_IO)   (Net DQS_t) (Diff_port 9)
Port 12  (Type S)(Physical C3)(Side Pad_IO)   (Net DQS_t) (Diff_port 10)

Port 13  (Type P)(Physical VDDQ)       (Side Pin_Rail)(Net VDDQ)
Port 14  (Type P)(Physical VDDQ_DIE-4) (Side Pad_Rail)(Net VDDQ)
Port 15  (Type P)(Physical VDDQ_DIE-8) (Side Pad_Rail)(Net VDDQ)
Port 16  (Type P)(Physical VDDQ_DIE-13)(Side Pad_Rail)(Net VDDQ)

Port 17  (Type P)(Physical VSS)        (Side Pin_Rail)(Net VSS) 
Port 18  (Type P)(Physical VSS_DIE-2)  (Side Pad_Rail)(Net VSS) 
Port 19  (Type P)(Physical VSS_DIE-6)  (Side Pad_Rail)(Net VSS) 
Port 20  (Type P)(Physical VSS_DIE-10) (Side Pad_Rail)(Net VSS)
[End Port Map]


Example 18: An IBIS on-die  [Interconnect Model] example using pad names and buffer terminals – without grouping (the model is between pad and buffer terminals).	Comment by Author: We may need to invent ways to refer to pad names and buffer terminals

[Begin Port Map]
Data_usage "IBIS_Interconnect"
Port 1   (Type S)(Physical A7)(Side Pad_IO)   (Net DM_n)
Port 2   (Type S)(Physical A7)(Side Buf_IO)   (Net DM_n)
Port 3   (Type P)(Physical A7)(Side Buf_PUref)(Net DM_n)
Port 4   (Type P)(Physical A7)(Side Buf_PDref)(Net DM_n)
Port 5   (Type S)(Physical C2)(Side Pad_IO)   (Net DQ0) 
Port 6   (Type S)(Physical C2)(Side Buf_IO)   (Net DQ0)
Port 7   (Type P)(Physical C2)(Side Buf_PUref)(Net DQ0) 
Port 8   (Type P)(Physical C2)(Side Buf_PDref)(Net DQ0) 
Port 9   (Type S)(Physical B7)(Side Pad_IO)   (Net DQ1) 
Port 10  (Type S)(Physical B7)(Side Buf_IO)   (Net DQ1)
Port 11  (Type P)(Physical B7)(Side Buf_PUref)(Net DQ1)
Port 12  (Type P)(Physical B7)(Side Buf_PDref)(Net DQ1)
Port 13  (Type S)(Physical D3)(Side Pad_IO)   (Net DQ2)
Port 14  (Type S)(Physical D3)(Side Buf_IO)   (Net DQ2)
Port 15  (Type P)(Physical D3)(Side Buf_PUref)(Net DQ2)
Port 16  (Type P)(Physical D3)(Side Buf_PDref)(Net DQ2)

Port 17  (Type S)(Physical B3)(Side Pad_IO)(Net DQS_c) (Diff_port 21)
Port 18  (Type S)(Physical B3)(Side Buf_IO)(Net DQS_c) (Diff_port 22)
Port 19  (Type P)(Physical B3)(Side Buf_PUref)(Net DQS_c)
Port 20  (Type P)(Physical B3)(Side Buf_PDref)(Net DQS_c)
Port 21  (Type S)(Physical C3)(Side Pad_IO)   (Net DQS_t) (Diff_port 17)
Port 22  (Type S)(Physical C3)(Side Buf_IO)   (Net DQS_t) (Diff_port 18)
Port 23  (Type P)(Physical C3)(Side Buf_PUref)(Net DQS_t)
Port 24  (Type P)(Physical C3)(Side Buf_PDref)(Net DQS_t)

Port 25  (Type P)(Physical VDDQ_DIE-4) (Side Pad_Rail)(Net VDDQ)
Port 26  (Type P)(Physical VDDQ_DIE-8) (Side Pad_Rail)(Net VDDQ)
Port 27  (Type P)(Physical VDDQ_DIE-13)(Side Pad_Rail)(Net VDDQ)

Port 28  (Type P)(Physical VSS_DIE-2) (Side Pad_Rail)(Net VSS)
Port 29  (Type P)(Physical VSS_DIE-6) (Side Pad_Rail)(Net VSS)
Port 30  (Type P)(Physical VSS_DIE-10)(Side Pad_Rail)(Net VSS)
[End Port Map]





BACKGROUND INFORMATION/HISTORY:

This change is intended for Touchstone 3.0.  It was developed by the IBIS Interconnect Task Group and approved on Month, Day, Year.
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