IBIS Measurement and Correlation Handbook outline – 23 March 2010

1)	Scope (Mike) Accuracy encompasses Construction, Measurement, and Correlation
2)	Definitions
3)	Measurement
i)	Measurement setup
(a)	Temperature and Voltage
(b)	Signal Types
1.	Single-ended
2.	Psuedo-differential
3.	True Differential
4.	Pre-emphasis
ii)	Measurement Quantities
(a)	Voltage/Time
(b)	Current/Time
(c)	Voltage/Current
(d)	Capacitance
iii)	Measurement methods
(a)	Simulation
1.	Reference simulator
2.	IBIS simulator
(b)	Bench Instrumentation
1.	Bare die
2.	Packaged part
3.	System
4)	Correlation
i)	Types of correlation metrics
(a)	Overlay validation
(b)	Envelope validation
(c)	Feature selective validation
1.	Frequency Domain (Bruce Archambeault)
2.	Voltage Domain
3.	Time Domain
ii)	I/V correlation
(a)	Driver I/V (Moshiul: frequently checked)
(b)	On-Die Termination I/V
(c)	Clamp I/V
iii)	V/T correlation
iv)	Input correlation
(a)	Effective capacitance
(b)	Reflection correlation
(c)	Receiver Output correlation ??? (not useful)
v)	Package correlation
(a)	Time of flight
(b)	Impedance
(c)	Frequency response
5)	Recommended Test Fixtures (Use [Test Load])
i)	Vref/Rref/Cref/Vmeas fixture
ii)	Differential fixtures